# FSSDE.Lynx_Winter_Compaction_Routes

## SDE Feature Class

Description | Spatial | Attributes

Keywords
Theme: Lynx, Habitat, Compaction
Description
Abstract

    Lynx Winter Compaction Routes

Purpose

    general location and reference.

Supplementary Information

    part of the official dataset provided to USFWS as required by the 2002 Revised Forest Plan.  Routes represent roads and trails that met the definition of compaction that was in use at the time of production.   Companion feature class is the Lynx_Winter_Compaction_Areas.

_________________
Status of the data
Complete
Data update frequency: Irregular
Time period for which the data is relevant
Date and time: 200305
Description:

    publication date

Publication Information
Who created the data: White River National Forest
Date and time: 200305
_________________
Data storage and access information
File name: FSSDE.Lynx_Winter_Compaction_Routes
Type of data: vector digital data
Location of the data:
- Server=oracle-idb.whiteriver.r2; Service=esri_sde; User=fssde; Version=FSSDE.FSSDE
Data processing environment: Microsoft Windows 2000 Version 5.0 (Build 2195) Service Pack 4; ESRI ArcCatalog 9.0.0.535
Accessing the data
Data format: ARCE
Constraints on accessing and using the data
Access constraints: The White River National Forest is the source of the most current version of this data. This data may be updated at any time without notifying previous recipients.
Use constraints:

    Data may be viewed and used by any and all entities upon request.  However, data may not be changed or modified in any way by anyone other than the originator.  The USDA-Forest Service does not guarantee the accuracy of this data

Details about this document
Contents last updated: 20060728 at time 16340700
Who completed this document
REQUIRED: The person responsible for the metadata information.
White River National Forest
mailing and physical address:

    900 Grand Avenue, PO Box 948

Glenwood Springs, Colorado 81602-0948
USA
(970) 945-2521 (voice)
(970) 945-3266 (fax)
Standards used to create this document
Standard name: FGDC Content Standards for Digital Geospatial Metadata
Standard version: FGDC-STD-001-1998
Time convention used in this document: local time
Metadata profiles defining additonal information
- ESRI Metadata Profile: http://www.esri.com/metadata/esriprof80.html
- ESRI Metadata Profile: http://www.esri.com/metadata/esriprof80.html
- ESRI Metadata Profile: http://www.esri.com/metadata/esriprof80.html
Horizontal coordinate system
Projected coordinate system name: NAD_1983_UTM_Zone_13N
Geographic coordinate system name: GCS_North_American_1983
Details
Grid Coordinate System Name: Universal Transverse Mercator
UTM Zone Number: 13
Transverse Mercator Projection
Scale Factor at Central Meridian: 0.999600
Longitude of Central Meridian: -105.000000
Latitude of Projection Origin: 0.000000
False Easting: 500000.000000
False Northing: 0.000000
Planar Coordinate Information
Planar Distance Units: meters
Coordinate Encoding Method: coordinate pair
Coordinate Representation
Abscissa Resolution: 0.010000
Ordinate Resolution: 0.010000
Geodetic Model
Horizontal Datum Name: North American Datum of 1983
Ellipsoid Name: Geodetic Reference System 80
Semi-major Axis: 6378137.000000
Denominator of Flattening Ratio: 298.257222
Altitude System Definition
Resolution: 1.000000
Encoding Method: Explicit elevation coordinate included with horizontal coordinates
_________________
Bounding coordinates
Horizontal
In decimal degrees
West: -108.026034
East: -105.775810
North: 40.216572
South: 38.955649
In projected or local coordinates
Left: 242356.739375
Right: 432812.279375
Top: 4452094.005000
Bottom: 4316060.005000
_________________
Lineage
FGDC lineage
Process step 1
Process description: Metadata imported.
Source used: C:\Documents and Settings\jevans\My Documents\metadata_template.xml
Process step 2
Process description: Metadata imported.
Source used: C:\gis\metadata\xml-sde\Wildlife\Lynx_Winter_Compaction_Areas.xml
Sources
Source 1
Media: Digital
Scale denominator: 40000
_________________
Spatial data description
Vector data information
ESRI description
FSSDE.Lynx_Winter_Compaction_Routes
ESRI feature type: Simple
Geometry type: Polyline
Topology: FALSE
Feature count: 2906
Spatial Index: TRUE
Linear referencing: FALSE
SDTS description
Feature class: SDTS feature type, feature count
- FSSDE.Lynx_Winter_Compaction_Routes: String, 2906
Details for FSSDE.Lynx_Winter_Compaction_Routes
Type of object: Feature Class
Number of records: 2906
Attributes
OBJECTID
Alias: OBJECTID
Data type: OID
Width: 4
Precision: 10
Scale: 0
Definition:

    Internal feature number.

Definition Source:

    ESRI

ID
Alias: ID
Data type: String
Width: 12
Precision: 0
Scale: 0
ACTION_
Alias: ACTION_
Data type: String
Width: 3
Precision: 0
Scale: 0
OTHER_SYSTEM
Alias: OTHER_SYSTEM
Data type: String
Width: 5
Precision: 0
Scale: 0
DATA_SOURCE
Alias: DATA_SOURCE
Data type: String
Width: 10
Precision: 0
Scale: 0
USE_LEVEL
Alias: USE_LEVEL
Data type: String
Width: 1
Precision: 0
Scale: 0
INCIDENTAL
Alias: INCIDENTAL
Data type: String
Width: 1
Precision: 0
Scale: 0
SM
Alias: SM
Data type: String
Width: 1
Precision: 0
Scale: 0
SC
Alias: SC
Data type: String
Width: 1
Precision: 0
Scale: 0
XC
Alias: XC
Data type: String
Width: 1
Precision: 0
Scale: 0
SS
Alias: SS
Data type: String
Width: 1
Precision: 0
Scale: 0
DS
Alias: DS
Data type: String
Width: 1
Precision: 0
Scale: 0
SB
Alias: SB
Data type: String
Width: 1
Precision: 0
Scale: 0
DH
Alias: DH
Data type: String
Width: 1
Precision: 0
Scale: 0
SL
Alias: SL
Data type: String
Width: 1
Precision: 0
Scale: 0
FT
Alias: FT
Data type: String
Width: 1
Precision: 0
Scale: 0
QUAD
Alias: QUAD
Data type: String
Width: 2
Precision: 0
Scale: 0
DESIGNATED
Alias: DESIGNATED
Data type: String
Width: 1
Precision: 0
Scale: 0
STATUS
Alias: STATUS
Data type: String
Width: 6
Precision: 0
Scale: 0
DES_METHOD
Alias: DES_METHOD
Data type: String
Width: 30
Precision: 0
Scale: 0
DES_LYNX
Alias: DES_LYNX
Data type: String
Width: 1
Precision: 0
Scale: 0
SHAPE
Alias: Shape
Data type: Geometry
Width: 4
Precision: 0
Scale: 0
Definition:

    Feature geometry.

Definition Source:

    ESRI

SHAPE.LEN
Alias: SHAPE.LEN
Data type: Double
Width: 0
Precision: 0
Scale: 0
MILES
Alias: MILES
Data type: Double
Width: 8
Precision: 38
Scale: 8
LYNX_EXEMPT
Alias: LYNX_EXEMPT
Data type: String
Width: 1
Precision: 0
Scale: 0